We use high resolution LED screen POLYLED P4, pixel pitch 4 mm.

|  |  |
| --- | --- |
| Pixel pitch | 4 mm |
| Resolution of cabinet | 128 х 128 pixels |
| Size of cabinet (W х H х D) | 512 х 512 х 105 mm |
| Best viewing angle | ≤ 140° |
| Brightness | > 1 400 cd/m² |
| Refresh frequence | > 2 000 Hz |
| Power consumption | < 950 W/m² |
| Working voltage | ~ 220 V/ 110 V ± 10% |
| Working temperature | -10°С ~45°С ± 10% |
| Weight of cabinet | 11, 4 kg. |

Screen is **7680 x 4096 mm**, total resolution is 1920 x 1024 px.